**ALU Code:-**

----------------------------------------------------------------------------------

-- Create Date: 28.08.2023 15:33:22

-- Design Name:

-- Module Name: ALU - Behavioral

-- Project Name:

-------------------------------------------------------------------------------

library IEEE;

use IEEE.STD\_LOGIC\_1164.ALL;

use IEEE.STD\_LOGIC\_unsigned.ALL;

-- Uncomment the following library declaration if using

-- arithmetic functions with Signed or Unsigned values

--use IEEE.NUMERIC\_STD.ALL;

-- Uncomment the following library declaration if instantiating

-- any Xilinx leaf cells in this code.

--library UNISIM;

--use UNISIM.VComponents.all;

entity ALU is

Port ( a : in STD\_LOGIC\_VECTOR (3 downto 0);

b : in STD\_LOGIC\_VECTOR (3 downto 0);

sel : in STD\_LOGIC\_VECTOR (3 downto 0);

y : out STD\_LOGIC\_VECTOR(3 downto 0));

end ALU;

architecture dataflow of ALU is

begin

y<=a when sel = "0000" else

a+1 when sel = "0001" else

a-1 when sel = "0010" else

b when sel = "0011" else

b+1 when sel = "0100" else

b-1 when sel = "0101" else

a+b when sel = "0110" else

a-b when sel = "0111" else

NOT a when sel = "1000" else

NOT b when sel = "1001" else

a AND b when sel = "1010" else

a OR b when sel = "1011" else

a NAND b when sel = "1100" else

a NOR b when sel = "1101" else

a XOR b when sel = "1110" else

a XNOR b when sel = "1111" ;

end dataflow;

**ALU Test Bench:-**

----------------------------------------------------------------------------------

-- Company:

-- Engineer:

--

-- Create Date: 28.08.2023 16:07:53

-- Design Name:

-- Module Name: ALU\_tb - Behavioral

-- Project Name:

-- Target Devices:

-- Tool Versions:

-- Description:

--

-- Dependencies:

--

-- Revision:

-- Revision 0.01 - File Created

-- Additional Comments:

--

----------------------------------------------------------------------------------

library IEEE;

use IEEE.STD\_LOGIC\_1164.ALL;

use IEEE.STD\_LOGIC\_unsigned.ALL;

-- Uncomment the following library declaration if using

-- arithmetic functions with Signed or Unsigned values

--use IEEE.NUMERIC\_STD.ALL;

-- Uncomment the following library declaration if instantiating

-- any Xilinx leaf cells in this code.

--library UNISIM;

--use UNISIM.VComponents.all;

entity ALU\_tb is

-- Port ( );

end ALU\_tb;

architecture beh of ALU\_tb is

COMPONENT ALU is

Port ( a : in STD\_LOGIC\_VECTOR (3 downto 0);

b : in STD\_LOGIC\_VECTOR (3 downto 0);

sel : in STD\_LOGIC\_VECTOR (3 downto 0);

y : out STD\_LOGIC\_VECTOR(3 downto 0));

end COMPONENT;

signal a,b,y: std\_logic\_vector(3 downto 0);

signal sel:std\_logic\_vector(3 downto 0):="0000";

begin

U1: ALU port map(a,b,sel,y);

process

begin

a<="1100";

b<="1010";

--sel<="0000";

--wait for 100 ns;


sel<=sel+1;

wait for 100 ns;

end process;

end beh;

**ALU O/P:-**

****